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WideSide® Sonar
{uithoptionalpurchase Wideide® transducer)

Your 700 Series™ fishing System also supparts
WideSide* sorar with the purchase of an additional
WideSide® transducer. The WideSice® transducer is 2
specalzed sidedooking”transducer that is extremely
usefulfor bank ishing o looking for bt ish in open
wiater The WideSide® transcucer uses three different
sonar elements that transmit signzls to the et rght
and straight down from your boat. The downward
beamis 200Kz witha 4" arez of coverage.This beam
mairtains acontinuous digtal depthreadout from the
Eottom irecty beneathyour bozt. Theside beams are
255 kHz with 16" area of coverage. The sidedooking
dements can be used independertl,or together to
locate targets near the surface of the water on ether
sdeof your boat.




